[English]
Warning: Only Support USB, if you want to read tag actively, you must use ReaderSoft to set interface to USB, and set WorkMode in ActiveMode. 

Compile with Eclipse2020, and java version is 1.8, and you should install windowbuilder in the eclipse

[Chinese]
提示：该代码仅适用于USB口。如果想要主动读卡，请用读卡器软件设置上传接口为USB，同时设置工作模式为 主动模式。

