[English]
Warning: Only Support USB Hid, if you want to read tag actively, you must use ReaderSoft to set interface to USB, and set WorkMode in ActiveMode. 

please copy libSWHidApi.so to system lib first
sudo  cp ~/libSWHidApi.so /lib/libSWHidApi.so

[Chinese]
提示：该代码仅适用于USB。如果想要主动读卡，请用读卡器软件设置上传接口为USB，同时设置工作模式为 主动模式。

please copy libSWHidApi.so to system lib first
sudo  cp ~/libSWHidApi.so /lib/libSWHidApi.so


