ActiveMode refers to the automatic card reading after the device is powered on, which is transmitted to the designated communication interface according to the set interface.
Interface can be USB,  RS232/RS485£¬ RJ45£¬ Keyboard£¬WIFI£¬ 4G, Bluetooth.
Keyboard is the virtual Keyboard output.

Use ReaderSoft ,  ParameterSet->Interface select  your interface such as RJ45,RS232.
then ParamterSet->WorkMde select ActiveMode.
